[image: ]ENVIRONMENTAL PROTECTION AGENCY
P.O. BOX 1439 WENO, CHUUKSTATE
FEDERATED STATES OF MICRONESIA
TEL: (691) 330-4158


Situation Report (SITREP)


SITREP No. 001	Name/contacts of person completing this report: C. R. Felix 

Date/time of SITREP: 04 – 15 – 2026/1444hrs	Date/time of incident: 04 – 11 – 2026/0300hrs – 0400hrs 

Location of incident: Latitude: 7º26’47.93” N Longitude: 151º50’22.77” E 

Description of location (e.g. name, distance and bearing to nearest landmark): Chuuk State Seaport – Weno, Chuuk

Nature and source of incident (indicate which of the following, identify vessels/specific source where possible): 

· Vessel aground/collision and leaking oil: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ 

· Vessel underway and discharging/leaking oil: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _  

· Vessel at anchor/moored/berthed and discharging/leaking oil: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ 

· Land-based source: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _  

· Oil slick with no definite source: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ 

· Other (please describe): 2 vessels aground – “Chief Mailo” & “Ballina”; “Chief Mailo” capsized – starboard side, oil sheen emanating from said vessel.

Visual appearance and extent of pollution (estimate area and quantity if possible): Oil sheen visible, emanating from capsized vessel (“Chief Mailo”), no emulsification yet; area coverage – 0.12 mi², estimate of 50 – 80 US gallons of marine diesel fuel.

Direction and rate of drift of pollution: North – northeast, drift rate @ 0.3 – 0.38 knots 
Wind speed & direction: 14kt – 15kt Southwind, Northward Sea state: WMO 4 (Moderate). Significant wave height 3’ – 5’. Small to moderate waves with occasional whitecaps. Residual swell from Typhoon SINLAKU diminishing.  Tide: Low tide 

Events since POLREP/last SITREP: _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ 

 (Attach additional information if required)
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Vessels Ballina & Chief Mailo grounded on the northern face of Chuuk State Seaport on Weno, Chuuk. Ballina (left side) grounded, but no visible oil leakage; Chief Mailo (right side) grounded & capsized on starboard side, oil sheen emanating from vessel.
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Shown in both pictures, starboard side of Ballina, no visible oil sheen or oil slick on water surface.
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All four pictures show the deck of Chief Mailo.
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Vessel shown is a 45 – foot fiberglass fishing boat grounded on the southeastern end of Fonoton. No visible oil slick, with minimal oil sheen due to fuel/lubricant residue within the vessel.
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